IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ProductLibraryView_V1.0]"
File name: "C:/Users/jvukovic/Desktop/Hansgrohe/IFC/xevolos_washbasin/61094-61094450-GLOSSY_WHITE-400Isometric_7.ifc"
Time stamp: "2023-03-09T07:35:02"
Originating system: "PARTsolutions"
Application: "PARTsolutions" version "V12.0" identifier "PARTsolutions" by Organization "Cadenas"

People and organizations
  Person "Cadenas" of Organization "Cadenas"
  Owner history of Person "Cadenas" of Organization "Cadenas" | application "PARTsolutions" version "V12.0" identifier "PARTsolutions" by Organization "Cadenas" | change ADDED | created 1678347302 (2023-03-09T07:35:02Z) | last modified 1678347302 (2023-03-09T07:35:02Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "61094-61094450-GLOSSY_WHITE-400"
  IFCSITE "SITE"
    contains 1 element
      1 x IFCDISCRETEACCESSORY | type IFCDISCRETEACCESSORYTYPE "61094-61094450-GLOSSY_WHITE-400" | names: "61094-61094450-GLOSSY_WHITE-400" | descriptions: "61094-61094450-GLOSSY_WHITE-400"

Types
  IFCDISCRETEACCESSORYTYPE "61094-61094450-GLOSSY_WHITE-400" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, ePset_PARTsolutions | description "61094-61094450-GLOSSY_WHITE-400"

Property sets
  Pset_DistributionPortCommon | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ColorCode (no value)
    PortNumber = 1 (IFCINTEGER)
  Pset_DistributionPortCommon | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ColorCode (no value)
    PortNumber = 2 (IFCINTEGER)
  Pset_DistributionPortTypePipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionSubType (no value)
    ConnectionType in {"UNSET"} (IFCLABEL)
    FlowCondition =  .. 
    InnerDiameter (no value)
    MassFlowRate =  .. 
    NominalDiameter = 46. (IFCLENGTHMEASURE) [MILLI METRE]
    OuterDiameter (no value)
    Pressure =  .. 
    Temperature =  .. 
    Velocity =  .. 
    VolumetricFlowRate =  .. 
  Pset_DistributionPortTypePipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionSubType (no value)
    ConnectionType in {"UNSET"} (IFCLABEL)
    FlowCondition =  .. 
    InnerDiameter (no value)
    MassFlowRate =  .. 
    NominalDiameter = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    OuterDiameter (no value)
    Pressure =  .. 
    Temperature =  .. 
    Velocity =  .. 
    VolumetricFlowRate =  .. 
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "61094450" (IFCIDENTIFIER)
    Manufacturer = "HANSGROHE" (IFCLABEL)
  ePset_PARTsolutions | properties | on 1 type object
    ARTNR = "61094450" (IFCTEXT)
    BASENUMBER = "61094" (IFCTEXT)
    BIMOBJECT = "Sanitary: Wash Basins" (IFCTEXT)
    CATALOG = "Hansgrohe" (IFCTEXT)
    DESCRIPTION = "Xevolos E Countertop basin ground 600/480 with tap hole without overflow, SmartClean" (IFCTEXT)
    DESIGN = "Germany" (IFCTEXT)
    DO = "46.000" (IFCTEXT)
    DOT = "35.000" (IFCTEXT)
    ETIM = "EC011550 | Washbasin" (IFCTEXT)
    GTINCODE = "4059625420850" (IFCTEXT)
    IFC = "Sanitary Terminal" (IFCTEXT)
    L = "600.000" (IFCTEXT)
    LI = "370.000" (IFCTEXT)
    LINA = "61094-61094450-GLOSSY_WHITE-400" (IFCTEXT)
    LODLEVEL = "400" (IFCTEXT)
    MANUFACTURER = "Germany" (IFCTEXT)
    MASTERFORMAT = "22 41 16.13 | Residential Lavatories" (IFCTEXT)
    MODEL = "61094XXX" (IFCTEXT)
    NAME = "Xevolos E Countertop basin ground 600/480 with tap hole without overflow, SmartClean" (IFCTEXT)
    NB = "61094-61094450-GLOSSY_WHITE-400" (IFCTEXT)
    NBSYN = "$BASENUMBER.-$ARTNR.-$SURFACE.-$LODLEVEL." (IFCTEXT)
    NN = "Xevolos Washbasin" (IFCTEXT)
    NT = "" (IFCTEXT)
    OBJECTTYPE = "Object (single object)" (IFCTEXT)
    OMNICLASS = "23-31 13 00 | Sinks" (IFCTEXT)
    PERMALINK = "61094XXX" (IFCTEXT)
    PRODUCTFAMILY = "Xevolos E" (IFCTEXT)
    PRODUCTGROUP = "Washbasins" (IFCTEXT)
    PRODUCTURL = "https://pro.hansgrohe.com/articledetail--61094450" (IFCTEXT)
    REGION = "Worldwide" (IFCTEXT)
    SPECIFICATION = "Surfaces: - 61094450 White Specification: " consists of: countertop basin ground, waste set, cover " material: ceramic " SmartClean: dirt-repellent glaze " degree of gloss: glossy " sanded basin underside " ceramic cover included " with one tap hole " without overflow " without shelf " non-closing waste set " 600 x 480 mm " type of installation: built on and wall mounted " suitable for cabinet" (IFCTEXT)
    SURFACE = "GLOSSY_WHITE" (IFCTEXT)
    TAP = "1" (IFCTEXT)
    TYP = "1" (IFCTEXT)
    UNICLASS2015 = "Pr_40_20_96 | Wash basins, sinks and troughs" (IFCTEXT)
    UNIFORMATII = "D2010 | Plumbing Fixtures" (IFCTEXT)
    UNSPSC = "301815 | Sanitary ware" (IFCTEXT)
    WEIGHT = "17" (IFCTEXT)
    X1 = "280.000" (IFCTEXT)
    X2 = "0.000" (IFCTEXT)