IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ProductLibraryView_V1.0]"
File name: "C:/Users/vklaic/AppData/Local/Temp/expmgtmp_10708_406.ifc"
Time stamp: "2023-09-13T12:34:54"
Originating system: "PARTsolutions"
Application: "PARTsolutions" version "V12.0" identifier "PARTsolutions" by Organization "Cadenas"

People and organizations
  Person "Cadenas" of Organization "Cadenas"
  Owner history of Person "Cadenas" of Organization "Cadenas" | application "PARTsolutions" version "V12.0" identifier "PARTsolutions" by Organization "Cadenas" | change ADDED | created 1694608494 (2023-09-13T12:34:54Z) | last modified 1694608494 (2023-09-13T12:34:54Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "toilet combinations-hansgrohe-62025XXX-EluPura S Wall hung WC Set 540 rimless AquaHelix Flush with WC seat and cover with SoftClose and QuickRelease, Slim, HygieneEffect"
  IFCSITE "SITE"
    contains 1 element
      1 x IFCDISCRETEACCESSORY | type IFCDISCRETEACCESSORYTYPE "62025-62025450-200" | names: "62025-62025450-200" | descriptions: "toilet combinations-hansgrohe-62025XXX-EluPura S Wall hung WC Set 540 rimless AquaHelix Flush with WC seat and cover with SoftClose and QuickRelease, Slim, HygieneEffect"

Types
  IFCDISCRETEACCESSORYTYPE "62025-62025450-200" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, ePset_PARTsolutions | description "toilet combinations-hansgrohe-62025XXX-EluPura S Wall hung WC Set 540 rimless AquaHelix Flush with WC seat and cover with SoftClose and QuickRelease, Slim, HygieneEffect"

Property sets
  Pset_DistributionPortCommon | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ColorCode (no value)
    PortNumber = 1 (IFCINTEGER)
  Pset_DistributionPortCommon | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ColorCode (no value)
    PortNumber = 2 (IFCINTEGER)
  Pset_DistributionPortTypePipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionSubType (no value)
    ConnectionType in {"UNSET"} (IFCLABEL)
    FlowCondition =  .. 
    InnerDiameter (no value)
    MassFlowRate =  .. 
    NominalDiameter = 102. (IFCLENGTHMEASURE) [MILLI METRE]
    OuterDiameter (no value)
    Pressure =  .. 
    Temperature =  .. 
    Velocity =  .. 
    VolumetricFlowRate =  .. 
  Pset_DistributionPortTypePipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionSubType (no value)
    ConnectionType in {"UNSET"} (IFCLABEL)
    FlowCondition =  .. 
    InnerDiameter (no value)
    MassFlowRate =  .. 
    NominalDiameter = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    OuterDiameter (no value)
    Pressure =  .. 
    Temperature =  .. 
    Velocity =  .. 
    VolumetricFlowRate =  .. 
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "62025450" (IFCIDENTIFIER)
    Manufacturer = "HANSGROHE" (IFCLABEL)
  ePset_PARTsolutions | properties | on 1 type object
    ARTNR = "62025450" (IFCTEXT)
    BASENUMBER = "62025" (IFCTEXT)
    BIMOBJECT = "Sanitary: Toilets" (IFCTEXT)
    CATALOG = "Hansgrohe" (IFCTEXT)
    COLLECTION = "toilet combinations" (IFCTEXT)
    COLLECTIONSET = "EluPura S" (IFCTEXT)
    DEPTH = "540.00" (IFCTEXT)
    DESCRIPTION = "EluPura S Wall hung WC Set 540 rimless AquaHelix Flush with WC seat and cover with SoftClose and QuickRelease, Slim, HygieneEffect" (IFCTEXT)
    DESIGN = "Germany" (IFCTEXT)
    GTINCODE = "4059625420942" (IFCTEXT)
    HEIGHT = "445.00" (IFCTEXT)
    IDNR = "1" (IFCTEXT)
    IFC = "Furnishing element" (IFCTEXT)
    LINA = "toilet combinations-hansgrohe-62025XXX-EluPura S Wall hung WC Set 540 rimless AquaHelix Flush with WC seat and cover with SoftClose and QuickRelease, Slim, HygieneEffect" (IFCTEXT)
    LODLEVEL = "200" (IFCTEXT)
    MANUFACTURER = "Germany" (IFCTEXT)
    MODEL = "62025XXX" (IFCTEXT)
    NAME = "EluPura S Wall hung WC Set 540 rimless AquaHelix Flush with WC seat and cover with SoftClose and QuickRelease, Slim, HygieneEffect" (IFCTEXT)
    NB = "62025-62025450-200" (IFCTEXT)
    NBSYN = "$BASENUMBER.-$ARTNR.-$LODLEVEL." (IFCTEXT)
    NN = "EluPura Q Wall hung WC Set 540 rimless with WC seat and cover with SoftClose and QuickRelease, HygieneEffect" (IFCTEXT)
    NT = "" (IFCTEXT)
    OBJECTTYPE = "Object (single object)" (IFCTEXT)
    OMNICLASS = "23-31 19 00 | Toilets" (IFCTEXT)
    PERMALINK = "62025XXX" (IFCTEXT)
    PRODUCTURL = "https://pro.hansgrohe.com/articledetail--62025450" (IFCTEXT)
    REGIONSET = "Worldwide" (IFCTEXT)
    SPECIFICATION = "Surfaces: - 62025450 White Specification: " consists of: WC, WC seat and cover, WC cover " material: ceramic " Made to fit NoiseReduction: customized soundproofing mat included " degree of gloss: glossy " type: Wall hung WC Set " with concealed siphon " rimless " HygieneEffect - reduces the spread of coliform bacteria and salmonella (Escherichia coli ATCC8739/Salmonella enterica ATCC 13076. Test: ISO 22196: 2011-08) " easy handling via push button " AquaHelix Flush: water vortex technology for optimal flushing " flushing type: wash-down " installation type: wall-mounted " concealed fastening for the WC " water connection: rear " with soft-close mechanism " QuickRelease: quick removable toilet seat and cover" (IFCTEXT)
    SURFACE = "white" (IFCTEXT)
    UNICLASS2015 = "Pr_40_20_93_94 | WC pans" (IFCTEXT)
    WEIGHT = "22" (IFCTEXT)
    WIDTH = "366.00" (IFCTEXT)